================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例配置LSI时钟从MCO（PA8）输出并将TIM14的通道1连接到MCO。将系统时钟配置为32MHz
（HSI 16MHz，PLL配置2倍频），TIM14时钟为320KHz，设置重载值为10001，使能TIM14的输入
捕获功能，调整LSI trimming值，LED亮起表示校准完成。

Function descriptions:
This example configures the LSI clock to output from MCO (PA8) and connects 
channel 1 of TIM14 to MCO. Set the system clock to 32MHz (HSI 16MHz, PLL 
frequency doubling), set the clock of TIM14 to 320KHz, set the overload value to
10001, enable the input capture function of TIM14, adjust the value of LSI 
trimming, and the LED ON indicates that calibration is complete.
================================================================================
测试环境：
测试用板：PY32F040E_STK
MDK版本： 5.28
IAR版本： 9.20
GCC 版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32F040E_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. 按下用户按键；
3. 等待LED亮起，用示波器监测PA08引脚上的频率，观察是否校准成功。

Example execution steps:
1. Compile and download the program to the MCU and run it.
2. Press the user button.
3. Wait for the LED to light up and monitor the frequency on the PA08 pin with 
an oscilloscope to see if the calibration is successful
================================================================================
注意事项：

Notes:

================================================================================
